18-2-6-4

18-2-6-3

18-2-3-4

                                                                                                              18-1-3-2

S0_SA_SB_CR

                                  8-1-2-1
                                   100NS

                                 S0_SA_SB

                                                      OUT2

                                                      OUT2

                                                      OUT1

                                                      OUT1

                                                        OUT

                                                   VETO

                                                   D

                                                   C

                                                   B

                                                   A

                                   P755

S0_CR

SB_CR

SA_CR

                                                                                                               18-1-4-3

                                                                                                                     18-1-10-8

OUT

OUTF

OUT

OUT

IN

                                                                                                                       P710

                                                                                                                     18-1-10-7

OUT

OUTF

OUT

OUT

IN

                                                                                                                       P710

BEAM.DT_CR

                                                                                                        8-3-9-2

                                                                                                   200MV

                                                                                                    20NS

OUT

OUTF

OUT

OUT

IN

                                                                                                         P710

                                                                                                        8-3-9-1

                                                                                                    200MV

                                                                                                     12NS

OUT

OUTF

OUT

OUT

IN

                                                                                                         P710

S0

                                                                                                                       [8-2-5-2]

                                                                                                                      [8-2-11-2] BEAM.DT

      BOS_CSI [5-1-9-7]

                                                                                      8-1-6-4
                                                                                       460NS

GATE

GATE

DEL

TTL

INH

OR

RESET

TRIG

                                                                                       P794

BM.DT_OR

                                                                                                                        [4-2-2-4]

     TCYL_AUX [8-2-6-1]

                                                                                           8-1-6-3
                                                                                          2MICROSEC

GATE

GATE

DEL

TTL

INH

OR

RESET

TRIG

                                                                                            P794

   LEV_1_TRIG [7-3-12-1] 8-1-6-2
                                                                                        1.74 MICROSEC

GATE

GATE

DEL

TTL

INH

OR

RESET

TRIG

                                                                                            P794

                                                                                                                        [5-1-11-5] TO_DAQ

CSI_TRIG

                                                                                                                        [5-1-9-4]

                  [7-5-10-1]
        CLR_BUSY
       LEV1_BUSY [7-5-10-2]
       LEV2_BUSY [7-5-10-3]

                  [8-1-5-4]
   TCYL_AUX_BUSY

                  [8-3-7-1]
        DAQ_BUSY

END_BSY

END_BSY

BUSY2

BUSY2

BUSY1

BUSY1

BUSY

BUSY

IN8

IN7

IN6

IN5

IN4

IN3

IN2

IN1

                                                                                               BUSY BOX

                                                                 TO_PLBY

                [8-1-3-2]

       DEADTIME (FM-7)

                                                8-2-9-1
                                                 200MV
                                                  10NS

                                               BEAM.DT

                                                                        IN

                                                                           OUT1

                                                                           OUT1

                                                 L821

                                                                           OUT2

                                                                            OUTF
                                                                            OUT

                                                                           OUT2

                                                                                                                      [7-1-1-2] UPST_BMTUN

                                          UPSTM_BM_TUNE

                                                8-1-2-2

                                           20NS

                                                                           OUT2

                                                                           OUT2

                                                                           OUT1

                                                                           OUT1

                                                                             OUT

                                                                        VETO

                                                                        D

                                                                        C

                                                                        B

                                                                        A

                                                 P755

                                                                                         16ns 16ns

                                                                     8-2-8-1

                                                                    BM.DT_OR

                                                                                                        A
                                                                                                        B
                                                                                                        C
                                                                                                        D OUT

                                                                                                           OUT2

                                                                                                           OUT2

                                                                                                           OUT1

                                                                                                           OUT1

                                                                      L429

                                                                                                            OUT

                                                                                     To MPS Clock Stop

                                                             8-1-4-1
                                                            1MICROSEC

                                                                                                 TTL

                                                                                                 DEL

                                                                                                 NIM

                                                                                                 NIM

                                                                                            BLNK

                                                                                            OR

                                                                                            STOP

                                                                                            STRT

                                                              L222

                                                               UPBM_TUNE_BUSY

                                                                      8-1-3-1

                                                                                                          A
                                                                                                          B
                                                                                                          C
                                                                                                          D OUT

                                                                                                             OUT2

                                                                                                             OUT2

                                                                                                             OUT1

                                                                                                             OUT1

                                                                       L429

                                                                                                              OUT

                   8-1-1-2

               33MV

                 8NS

                              IN

                                 OUT1

                                 OUT1

                     L821

                                 OUT2

                                  OUTF
                                  OUT

                                 OUT2

UPST_SEL

        [4-1-1-2]

                                                                                                                     [7-1-3-1]

                                                  8-1-4-2
                                                 1MICROSEC

                                                                                 TTL

                                                                                 DEL

                                                                                 NIM

                                                                                 NIM

                                                                            BLNK

                                                                            OR

                                                                            STOP

                                                                            STRT

                                                   L222

                                                            8-1-3-4

                                                                                            A
                                                                                            B
                                                                                            C
                                                                                            D OUT

                                                                                               OUT2

                                                                                               OUT2

                                                                                               OUT1

                                                                                               OUT1

                                                              L429

                                                                                                OUT

                                                                                                  8-3-9-3

                                                                                             200MV

                                                                                               20NS

                  8-1-1-3

             185MV

               35NS

                            IN

                               OUT1

                               OUT1

                   L821

                               OUT2

                                OUTF
                                OUT

                               OUT2

                  8-1-1-1

              50MV

              30NS

                            IN

                               OUT1

                               OUT1

                   L821

                               OUT2

                                OUTF
                                OUT

                               OUT2

                                                      5-1-9-4

                                                 150MV

                                                   40NS

                                                                                        OUT

                                                                                       OUTF

                                                                                       OUT

                                                                                       OUT

                                                                                   IN

                                                        P710

                                                    8-1-6-1

                                                 CSI_GATE_DELAY
                                               240NS

                                                                                    GATE

                                                                                    GATE

                                                                                     DEL

                                                                                     TTL

                                                                              INH

                                                                              OR

                                                                              RESET

                                                                              TRIG

                                                     P794

                                 8-1-2-4

                                   CSI
                              20NS

                                                      OUT2

                                                      OUT2

                                                      OUT1

                                                      OUT1

                                                        OUT

                                                   VETO

                                                   D

                                                   C

                                                   B

                                                   A

                                   P755

                  8-1-1-4

             200MV

              130NS

                             IN

                                OUT1

                                OUT1

                    L821

                                OUT2

                                 OUTF
                                 OUT

                                OUT2

(FM-1) FTBUSY

S0_TDC

[8-2-1-15]

                                                                                                                     8-1-5-3

                                                                                                                     CSI_GATE

A
B
C
D OUT

OUT2

OUT2

OUT1

OUT1

                                                                                                                       L429

OUT

     BUSY, CSI AND BEAM TUNE

       CSI_AUX
        [10-1-2-3]

CSI_GATE
[10-3-11-4]

                                         S

                                                         CSI_BUSY FT_BUSY

                  [8-1-3-2]

      CSI_SWITCH [7-2-8-1]

                                                                                  TO PRETRIGGER STROBES

                                                                                         TO PRETRIGGER

           FROM LEVEL1 PRESCALE

          SAPM

           SBPM

         S0PM

                                                                                               TO TAGS

OUT

OUTF

OUT

OUT

IN

                                                                                                                P710

                                                                                                             18-1-2-6

OUT3

OUT2

OUT1
IN

                                                                                                              L623B

                                                                                                 7-5-11

A
B
C
D OUT

OUT2

OUT2

OUT1

OUT1

                                                                                                            L429

OUT

                                                                                                          7-5-12-1

AUX

  GLOBAL_BUSY

     GLOBAL_BUSY

OUT

OUTF

OUT

OUT

IN

                                                                                                   P710

OUT3

OUT2

OUT1
IN

                                                                                                                 L623B

OFLO

SCLR

IN

                                                                                                                       18-2-3-3^{IN}

SCLR

OFLO

SCLR

IN IN

SCLR

         13 FEBRUARY 1995