                                                                                              STRB_LEV2_SCLR

                                                                                               7-5-2-4

                                                                                                                8-5-11-3 LEV2_BUSY

                                                                                                                   8-5-11-1 CLR_BUSY

8-2-12

      7-5-4

      LEV_2D

LEVEL2_FINAL_TRIG
   18-JULY-94

             Q4

             Q4Q4

             Q3Q3

             Q3Q2

             Q2

             Q2Q1

             Q1Q1

        I3

        I2

        I1

        I0

      ECLL4616_{NIM}

                                                                                                               TDC_CAT_CLR

                                                                                                          TCYL_CLR?

Q3

Q2

Q1

Q0

I3

I2

I1

I0 ECL

NIML4616

104-8

HODO

TDX4

Q3

Q2

Q1

Q0

I3

I2

I1

I0 ECL

NIML4616

                                                                                                    TCYL_CLR

                                                                                                 CLR_BUSY

                                                                                                 7-5-10-1^{GATE}

GATE

DEL

TTL

INH

OR

RESET

TRIG

                                                                                                   P794

                                                                                                 8-2-8-3

                                                                                                 CLEAR_FO

A
B
C
D OUT

OUT2

OUT2

OUT1

OUT1

                                                                                                   L429

OUT

                                                                                                LEV2_CLR_FO

                                                                                                 7-5-7-4

A
B
C
D OUT

OUT2

OUT2

OUT1

OUT1

                                                                                                   L429

OUT

                                                                     7-5-7-2

                                                                     CLEAR_OR

                                                                                                         A
                                                                                                         B
                                                                                                         C
                                                                                                         D OUT

                                                                                                            OUT2

                                                                                                            OUT2

                                                                                                            OUT1

                                                                                                            OUT1

                                                                       L429

                                                                                                             OUT

                                                                    CSI_CLR

                                            LEV1_CLR
                                            7-3-12-2

                                                                       8-3-5

                                                                                                                 Q3

                                                                                                                 Q2

                                                                                                                 Q1

                                                                                                                 Q0

                                                                                                           I3

                                                                                                           I2

                                                                                                           I1

                                                                                                           I0 ECL

                                                                        NIML4616

                                                                     DAQ_INPUT

                                                                                DAQ_INTERFACE

                                                                                                                 Q3

                                                                                                                 Q2

                                                                                                                 Q1

                                                                                                                 Q0

                                                                                                           I3

                                                                                                           I2

                                                                                                           I1

                                                                                                           I0 ECL

                                                                        NIML4616

                                                                 7-5-12-3

                                                               FINAL_TRG_OR

                                                                                                   A
                                                                                                   B
                                                                                                   C
                                                                                                   D OUT

                                                                                                      OUT2

                                                                                                      OUT2

                                                                                                      OUT1

                                                                                                      OUT1

                                                                   L429

                                                                                                       OUT

                                                       SSP0_OR_PULSER

                                                                                                         8-2-8-4

                                                                                                        TDC_STOP_FO

A
B
C
D OUT

OUT2

OUT2

OUT1

OUT1

                                                                                                          L429

OUT

                                                                        8-4-3-1

                                                                          SSP0

                                                                                                             IN

                                                                                                                OUT1

                                                                                                                OUT1

                                                                          L821

                                                                                                                OUT2

                                                                                                                 OUTF
                                                                                                                 OUT

                                                                                                                OUT2

                                                                               SSP0_STRETCH

                                                                                  8-3-4-3^{GATE}

GATE

DEL

TTL

INH

OR

RESET

TRIG

                                                                                   P794
             2AB_CHRG_STRETCHER

               8-4-1-3^{GATE}

                            GATE

                             DEL

                             TTL

                      INH

                      OR

                      RESET

                      TRIG

                P794

                                                                                           TCYL_TDX4

                                                                                            8-2-11-1

                                                                                            TDC_STOP

OUT2

OUT2

OUT1

OUT1

OUT

VETO

D

C

B

A

                                                                                              P755
                                                                             FINAL_TRG_DLY

                                                                                8-2-10-1^{TTL}

DEL

NIM

NIM

BLNK

OR

STOP

STRT

                                                                                  L222

              MAM_DLY_300

            2D_NEUT
            LINE_15

            2C_NEUT
            LINE_7

            2D_CHG
            LINE_16

             2C_CHG
             LINE_8

                                                        LEV2_CLEAR

                                                       7-5-6-2

                                                                                       OUT2

                                                                                       OUT2

                                                                                       OUT1

                                                                                       OUT1

                                                                                         OUT

                                                                                    VETO

                                                                                    D

                                                                                    C

                                                                                    B

                                                                                    A

                                                         P755

                         7-5-5-1

                         CHARGED

                                     A
                                     B
                                     C
                                     D OUT

                                        OUT2

                                        OUT2

                                        OUT1

                                        OUT1

                          L429

                                         OUT

                                        7-5-4-3

                                     CHG_OR_NEUT

                                                            A
                                                            B
                                                            C
                                                            D OUT

                                                               OUT2

                                                               OUT2

                                                               OUT1

                                                               OUT1

                                         L429

                                                                OUT

                                                                     7-2-3-3

                                                                                                       IN

                                                                      SCLR

                                                                 7-5-10-3

                                                               LEV2_BUSY

                                                                                                       GATE

                                                                                                       GATE

                                                                                                        DEL

                                                                                                        TTL

                                                                                                 INH

                                                                                                 OR

                                                                                                 RESET

                                                                                                 TRIG

                                                                  P794

                                                    SPILL_ENABLE
                                                                    1

                                                    4_LGD_PULSER_TRG CABLE 23

                                                                 3

                                                                     2

                                                         8-3-3-1

                                                       DAQ_INPUT

                                                                                            OUT

                                                                                           OUTF

                                                                                           OUT

                                                                                           OUT

                                                                                       IN

                                                           P710

                                                          8-3-3-2^{OUT}

                                                                                           OUTF

                                                                                           OUT

                                                                                           OUT

                                                                                       IN

                                                           P710

                                              7-5-6-3

                                            CHG_TO_DAQ

                                                                        OUT2

                                                                        OUT2

                                                                        OUT1

                                                                        OUT1

                                                                          OUT

                                                                     VETO

                                                                     D

                                                                     C

                                                                     B

                                                                     A

                                               P755

                                            NEUT_TO_DAQ

                                             7-5-6-4

                                                                        OUT2

                                                                        OUT2

                                                                        OUT1

                                                                        OUT1

                                                                          OUT

                                                                     VETO

                                                                     D

                                                                     C

                                                                     B

                                                                     A

                                               P755

                                                   7-5-6-1

                                                   LEV2_TRIG

                                                                                 OUT2

                                                                                 OUT2

                                                                                 OUT1

                                                                                 OUT1

                                                                                   OUT

                                                                              VETO

                                                                              D

                                                                              C

                                                                              B

                                                                              A

                                                     P755

                        NEUTRAL

                        7-5-5-2

                                     A
                                     B
                                     C
                                     D OUT

                                        OUT2

                                        OUT2

                                        OUT1

                                        OUT1

                          L429

                                         OUT

      7-5-4

     LEV_2C

             Q4Q4

             Q4

             Q3Q3

             Q3

             Q2Q2

             Q2Q1

             Q1Q1

        I3

        I2

        I1

        I0

      ECLL4616_{NIM}

     8-4-6

      2A&2B
    CHARGED_OR
      L429

            OUT7

            OUT7

            OUT5

            OUT5

            OUT3

            OUT3

            OUT1

            OUT1

            OUT8

            OUT8

            OUT7

            OUT7

            OUT6

            OUT6

            OUT5

            OUT5

            OUT4

            OUT4

            OUT3

            OUT3

            OUT2

            OUT2

            OUT1

            OUT1

        P

        O

        N

        M

        L

        K

        J

        I

        H

        G

        F

        E

        D

        C

        B

        A

                                    MAM_DLY_300

Q3

Q2

Q1

Q0

I3

I2

I1

I0 ECL

NIML4616

Q3

Q2

Q1

Q0

I3

I2

I1

I0

ECL

NIML4616

A
B
C
D OUT

OUT2

OUT2

OUT1

OUT1

                                                                                                 L429

OUT