                 8-1-7-1
                  200MV

                               OUT

                              OUTF

                             OUT2

                             OUT2

                             OUT1

                             OUT1

                          IN

                 L621BL

                                                                                     300NS

                                                                                   8-4-1-2

                                       MAMM STROBES LEVEL 2
                                      IF PULSER OR BYPASS ON
                                      STROBE IS PRETRIG DELAYED

GATE

GATE

DEL

TTL

INH

OR

RESET

TRIG

                                                                                     P794

 FROM HUT

                               14 JANUARY 1995

                              MAM DONE STROBES

                                                                                          TO LEVEL 2 MLU

                                                                                     TO LEVEL 2 PRESCALE

                                                                                               MAM_DLY_300

                                                                                                 7-5-7-1

A
B
C
D OUT

OUT2

OUT2

OUT1

OUT1

                                                                                                   L429

OUT

                                                                                                       7-5-5-4

A
B
C
D OUT

OUT2

OUT2

OUT1

OUT1

                                                                                                        L429

OUT

                                                                                                     MAM_DLY_150

                                                                                                       7-5-2-3

A
B
C
D OUT

OUT2

OUT2

OUT1

OUT1

                                                                                                         L429

OUT

                                                                                                                        [7-4-9-2] CLR_LEV2

STRB_LEV2

                                                                                                                        [7-4-9-1]

                                                                                                                        [7-4-9-1] CLR_LEV2

                                                                                                                        [7-4-9-2] STRB_LEV2

                                                                                                                  [7-5-6-3] MAM_DLY_301
                                                                                                                  [7-5-6-4] MAM_DLY_301

                                                                                                                  [7-5-6-1] MAM_DLY_300
                                                                                                                  [7-5-6-2] MAM_DLY_300

                                                                                TO LEVEL 2 FINAL TRIGGER

                                                                                          TO LEVEL 2 MLU

                                                                                           13
                                                                                           14
                                                                                           15
                                                                                           16
                                                                                               7-1-7

Q3

Q2

Q1

Q0

I3

I2

I1

I0

ECL

                                                                                                NIML4616

LEV2_STRBD

                                                                                                                   [7-4-7]

LEV2_STRBB

                                                                                                                   [7-4-2]

LEV2_STRBA

                                                                                                                   [7-4-1]

LEV2_STRBC

                                                                                                                   [7-4-6]

                                                                               LEV2_STROBE

                                                                                7-3-12-3

A
B
C
D OUT

OUT2

OUT2

OUT1

OUT1

                                                                                  L429

OUT

LEV2_LTCH_STRB

                                                                                                                 [7-4-21-2]

                                                                                                        MAM_DONE

                                                                                                       7-5-12-2

A
B
C
D OUT

OUT2

OUT2

OUT1

OUT1

                                                                                                         L429

OUT

LEV2_LTCH_CLR

                                                                                                                  [7-4-21-2]

LEV2_LTCH_CLR

                                                                                                                  [7-4-21-1]

                SWITCH
             MAMM_BYPASS

LEV2_LTCH_STRB

                                                                                                                 [7-4-21-1]

         (FH-13)
MAM_DONE

       [3-1-23]
MB_SW

                                                                                     MAM_DLY_150

                                                                                      7-5-12-4

A
B
C
D OUT

OUT2

OUT2

OUT1

OUT1

                                                                                         L429

OUT

                                                                              150 NS

                                                                            8-4-1-1

GATE

GATE

DEL

TTL

                                                                                                                   INH

                                                                                                                   OR

                                                                                                                   RESET

                                                                                                                   TRIG

                                                                              P794

                                                                                               A
                                                                                               B
                                                                                               C
                                                                                               D OUT

                                                                                                  OUT2

                                                                                                  OUT2

                                                                                                  OUT1

                                                                                                  OUT1

                                                                L429

                                                                                                   OUT

                                                            MAMM_DONE_OR

                                                     10US

                                                   8-1-9-1

                                                                                   GATE

                                                                                   GATE

                                                                                    DEL

                                                                                    TTL

                                                                             INH

                                                                             OR

                                                                             RESET

                                                                             TRIG

                                                     P794

                                        LEV1_TRG

                                          8-1-8-2

                                                                  OUT2

                                                                  OUT2

                                                                  OUT1

                                                                  OUT1

                                                                    OUT

                                                               VETO

                                                               D

                                                               C

                                                               B

                                                               A

                                           P755

          [7-3-12-1]
LEV1_TRG

                              SWITCH
                                 OR

                              8-1-10-4

                                              A
                                              B
                                              C
                                              D OUT

                                                 OUT2

                                                 OUT2

                                                 OUT1

                                                 OUT1

                               L429

                                                  OUT

                                     MAMM*/SWITCH

                                      8-1-8-1

                                                             OUT2

                                                             OUT2

                                                             OUT1

                                                             OUT1

                                                               OUT

                                                          VETO

                                                          D

                                                          C

                                                          B

                                                          A

                                       P755

              8-1-10-2

                       A
                       B
                       C
                       D OUT

                          OUT2

                          OUT2

                          OUT1

                          OUT1

                L429

                           OUT

         [8-1-5-1]
 PLSR_SW

                 SWITCH

                          A
                          B
                          C
                          D OUT

                             OUT2

                             OUT2

                             OUT1

                             OUT1

                  L429

                              OUT

               SYS_PULSER

                                                              8-1-10-1

                8-1-10-3_{50ns}