                                                                                                     AND 1 HIT IN D

                                                                                                HITS IN A B AND C AND

                                                                                                      MAY 22 1997

                                                                                                  TCYL MULTIPLICITY

                                                                                  TCYL EQ 1
                                                                     D LE 1

                                                                      D GE 1

                                                                    ALL GE 1

                                                MULT GE 2

                                                 MULT OR

                                                 LATCH OR

                             GE 2

                             GE 2

                             GE 2

                               FIN OUT

                              GE 2

                        IU MULT UNITS

                                                                                              HITS IN THE D LAYER

                                                                                           TCYL_GT0 MEANS 1 OR MORE

                                                                                 OUT

                                                   L429_{OUT1}

                                                                                OUT1
                                                                                OUT2
                                                                                OUT2
                                                                                 OUT

                                                                             D

                                                                             C

                                                                             B

                                                                             A

                                                                                 OUT

                                                   L429_{OUT1}

                                                                                OUT1
                                                                                OUT2
                                                                                OUT2
                                                                                 OUT

                                                                             D

                                                                             C

                                                                             B

                                                                             A

                                                                                 OUT

                                                   L429_{OUT1}

                                                                                OUT1
                                                                                OUT2
                                                                                OUT2
                                                                                 OUT

                                                                             D

                                                                             C

                                                                             B

                                                                             A

                                                                                 OUT

                                                   L429_{OUT1}

                                                                                OUT1
                                                                                OUT2
                                                                                OUT2
                                                                                 OUT

                                                                             D

                                                                             C

                                                                             B

                                                                             A

OUT

OUT2

OUT2

OUT1

OUT1

VETO

D

C

B

A

                                                                                            C314

                                                                                         23-2-12-2

                                                                                                     23-2-12-1

                                                 23-2-10

                                                  23-2-7

                                                                                                                   TCYL_GT0

                                                                                                      [7-1-1-3]

LTCH_GAT2 [23-1-8-2]

LTCH_GAT1 [23-1-8-2]

50ns 50ns 50ns

50ns

                                                                                                                       50ns

                                                                                 OUT

                                                   L429_{OUT1}

                                                                                OUT1
                                                                                OUT2
                                                                                OUT2
                                                                                 OUT

                                                                             D

                                                                             C

                                                                             B

                                                                             A

               50

               50

                            50

LTCH_CLR [23-1-12-4]

                                                                     UNCLIPPED

                                                                    IN=1_2_3_4

                                                                      LEV=4

                                                                     23-2-8-1

16ns

                                                                       IN=4

                                                                      LEV=1
                                                                    UNCLIPPED

                                                                     23-2-8-2

                                                                      LEV=1
                                                                      IN=4
                                                                   UNCLIPPED

                                                                    23-2-9-2

                                                                                    LEV=2
                                                                                  UNCLIPPED

                                                                                  23-2-9-1

                                                                                   IN=1_2

                           A-LAYER

                           22-5-3
                           B-LAYER

                            22-5-7

                           C-LAYER

                           22-5-11
                           D-LAYER

                           22-5-15

                                         GATE
                                         GATE

                                         RESET
                                         RESET

                                               F_OR
                                               F_OR

                                               LTCH
                                               LTCH

                                        I1
                                        I2I3
                                        I4I5
                                        I6I7
                                        I8
                                        I9I10
                                        I11I12
                                        I13I14
                                        I15I16

                          MULT_LTCH

                                         GATE
                                         GATE

                                         RESET
                                         RESET

                                               F_OR
                                               F_OR

                                               LTCH
                                               LTCH

                                        I1I2
                                        I3I4
                                        I5I6
                                        I7I8
                                        I9
                                        I10I11
                                        I12I13
                                        I14I15
                                        I16

                          MULT_LTCH

                                         GATE
                                         GATE

                                         RESET
                                         RESET

                                               F_OR
                                               F_OR

                                               LTCH
                                               LTCH

                                        I1I2
                                        I3I4
                                        I5I6
                                        I7
                                        I8I9
                                        I10I11
                                        I12I13
                                        I14I15
                                        I16

                          MULT_LTCH

                                         GATE
                                         GATE

                                         RESET
                                         RESET

                                               F_OR
                                               F_OR

                                               LTCH
                                               LTCH

                                        I1I2
                                        I3I4
                                        I5I6
                                        I7I8
                                        I9
                                        I10I11
                                        I12I13
                                        I14I15
                                        I16

                          MULT_LTCH

                                                                                 OUT

                                                   L429_{OUT1}

                                                                                OUT1
                                                                                OUT2
                                                                                OUT2
                                                                                 OUT

                                                                             D

                                                                             C

                                                                             B

                                                                             A

                                                                                 OUT

                                                   L429_{OUT1}

                                                                                OUT1
                                                                                OUT2
                                                                                OUT2
                                                                                 OUT

                                                                             D

                                                                             C

                                                                             B

                                                                             A

                                                                                 OUT

                                                   L429_{OUT1}

                                                                                OUT1
                                                                                OUT2
                                                                                OUT2
                                                                                 OUT

                                                                             D

                                                                             C

                                                                             B

                                                                             A

                                                                                                                OUT

                                                                                                              OUT2

                                                                                                              OUT2

                                                                                                              OUT1

                                                                                                              OUT1

                                                                                                           VETO

                                                                                                           D

                                                                                                           C

                                                                                                           B

                                                                                                           A

                                                                       J101

                                                                                                                OUT

                                                                                                              OUT2

                                                                                                              OUT2

                                                                                                              OUT1

                                                                                                              OUT1

                                                                                                           VETO

                                                                                                           D

                                                                                                           C

                                                                                                           B

                                                                                                           A

                                                                       J101

                                                                                                              OUT

                                                                                                            OUT2

                                                                                                            OUT2

                                                                                                            OUT1

                                                                                                            OUT1

                                                                                                         VETO

                                                                                                         D

                                                                                                         C

                                                                                                         B

                                                                                                         A

                                                                      J101

OUT

OUT2

OUT2

OUT1

OUT1

VETO

D

C

B

A

                                                                                    J101

OUT

OUT2

OUT2

OUT1

OUT1

VETO

D

C

B

A

                                                                                                        C314

16ns TCYL_EQ1

                                                                                             TCYL_EQ1 MEANS ONE OR MORE

                                                                                                        [7-1-1-4]